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15-Inch Full Flat Fanless POS System
TP-1115
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Features
· ARM Quad-core ARM Cortex-A17 32-bit processor
· True-Flat Projected Capacitive Multi Touch and True-Flat 5-wire Resistive Touch supported
· Excellent ergonomic and simple design
· Module architecture for efficient chassis integration
· Modular motherboards with hard drives can be easily extracted replacement
· Communication : Wi-Fi and 4G LTE supported (Optional)
· OS : Android 7.1
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Specifications
	Model Name
	TP-1115

	Processor
	Quad-core ARM Cortex-A17 MPCore  up to 1.8GHz

	CPU
	Mali-T764 GPU

	Memory
	2GB DDR3

	Storage
	16GB eMMC
1 x microSD Slot

	LCD Panel
	15-inch TFT LCD with LED Backlight

	
	1024 (W) RGB x 768 (H)

	Touch Panel
	 True-Flat Projected Capacitive Multi Touch

	
	True-Flat 5-wire Resistive Touch

	Speaker
	1 x 2W High Quality Speaker

	I/O Expansion

	USB
	7 x USB Type A

	OTG
	1 x USB Type A

	LAN
	1 x RJ45 10/100/1000Mbps Giga Ethernet

	COM
	COM3 (DB9), w/ +5V by Jump

COM4 (RJ45), w/ +5V/12V by Jump

	HMDI
	1 x HDMI

	Audio
	1 x Line-out

	Cash Drawer
	1 x RJ11 port supports 1 cash drawer with 12V

	DC Power Out
	1 x +12V Power Out

	DC Power In
	1 x Standard Mini-DIN 4PIN type

	Power Management

	Power Adapter
	12V@5.0A, 60W Adapter

	Mechanical & Environmental

	Dust and Water
	IP65 on Front Panel

	Tilt Adjustment
	15° ~ 85 °

	Dimension
	355 (W) x 303 (H) x 205 (D) mm

	Weight
	4.3 kg

	Certification
	CE/FCC/LVD

	Operation System
	Android 7.1

	Operation Condition
	0°C to +40°C / 20 to 80% without condensation

	Storage Condition
	-20°C to +55°C / 20 to 85% without condensation

	Optional Accessories

	Customer Display
	VFD and LCD Customer Display

	MSR
	Comply with ISO 7811 and Three Track support

	Combo Card Reader
	MSR - Comply with ISO 7811/JSII and Three Track

RFID - Comply Mifare, ISO14443AB-4 and Felica

	i-Button
	Dallas i-button Reader

	Wi-Fi
	Wi-Fi IEEE 802.11 b/g/n

	4G LTE
	4G LTE Mini-PCIe with External Antenna Rod

	VESA Bracket
	VESA-Compatible, 75 x 75 (mm)
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